Engine CHT and Oil temperatures after a flight using cowl plugs to retain heat.

Note that the oil temperature is recorded from the standard sensor located at the rear of the engine, it is not located in the oil sump. Also, it is not recorded below 75 degF. The ambient temperature was about 34 degF.